{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B (Archived)","FTXTM40M2V1B (Archived)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.032","0.037"]
["","Chauffage","","Nom.","kW","0.037","0.04"]
["Caisson","Couleur","","","","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","294","300"]
["","","","Largeur","mm","811","1040"]
["","","","Profondeur","mm","272","295"]
["Poids","Unité","","","kg","10","14.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","11.7","15.5"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","8","9.2"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","6.3","5.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","5.2","4.6"]
["","","Chauffage","Haut","m³/min","12.2","17.7"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","7.5","11"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.1","7.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1","6.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60","60"]
["","Chauffage","","","dBA","61","61"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","45","46"]
["","Refroidissement","","Moyen","dBA","33","32"]
["","","","Bas","dBA","25","24"]
["","","","Faible niveau sonore de fonctionnement","dBA","21","20"]
["","Chauffage","","Haut","dBA","45","46"]
["","","","Moyen","dBA","31","31"]
["","","","Bas","dBA","22","22"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5"]
["","Évacuation","","","","16 (diamètre interne du flexible de raccordement)","16 (diamètre interne du flexible de raccordement)"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A55","ARC466A55"]
["","Télécommande câblée","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Alimentation électrique","Nom","","","","V1","V1"]
["","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]