{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","45.0"]
["","","","Moyen","dBA","31.0"]
["","","","Faible niveau sonore de fonctionnement","dBA","19.0"]
["","","","Bas","dBA","22.0"]
["","Rafraîchissement","","Moyen","dBA","33.0"]
["","","","Faible niveau sonore de fonctionnement","dBA","21.0"]
["","","","Bas","dBA","25.0"]
["","","","Haut","dBA","45.0"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Manuel d’utilisation","","","","1"]
["","Télécommande infrarouge","","","","1"]
["","Piles sèches AAA","","","","2"]
["","Support de télécommande","","","","1"]
["","Plaque de montage","","","","1"]
["","Vis de fixation d'unité intérieure","","","","2"]
["","Filtre à particules argent","","","","1"]
["Systèmes de commande","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35"]
["","Gaz","","DE","mm","9.50"]
["","Drain","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.035"]
["","Chauffage","","Nom.","kW","0.039"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60.0"]
["","Chauffage","","","dBA","61.0"]
["Dimensions","Unité","","Largeur","mm","778"]
["","","","Profondeur","mm","272"]
["","","","Hauteur","mm","295"]
["Caisson","Colour","","","","Blanc"]
["Poids","Unité","","","kg","10.0"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","12.5"]
["","","","Bas","m³/min","4.9"]
["","","","Moyen","m³/min","7.5"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.0"]
["","","Rafraîchissement","Bas","m³/min","5.3"]
["","","","Moyen","m³/min","7.8"]
["","","","Haut","m³/min","12.2"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1"]
["Power supply","Phase","","","","1~"]
["","Fréquence","","","Hz","50"]
["","Nom","","","","V1"]
["","Tension","","","V","220-240"]
["Remarques","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19,0 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m"]
["","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["","","","","","(3) - Pour les données électriques, se reporter aux schémas séparés."]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.053"]
["","Chauffage","","Nom.","kW","","0.06"]
["Caisson","Couleur","","","","","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","299"]
["","","","Largeur","mm","","998"]
["","","","Profondeur","mm","","292"]
["Poids","Unité","","","kg","","14.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","15.4"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","9.5"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","5.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.6"]
["","","Chauffage","Haut","m³/min","","17.5"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","10.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","7.1"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","5.9"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","60"]
["","Chauffage","","","dBA","","61"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","46"]
["","Refroidissement","","Moyen","dBA","","32"]
["","","","Bas","dBA","","24"]
["","","","Faible niveau sonore de fonctionnement","dBA","","20"]
["","Chauffage","","Haut","dBA","","46"]
["","","","Moyen","dBA","","31"]
["","","","Bas","dBA","","22"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35"]
["","Gaz","","DE","mm","","9.5"]
["","Évacuation","","","","","18"]
["Systèmes de commande","Infrared remote control","","","","","ARC466A75"]
["Systèmes de commande","Télécommande câblée","","","","","BRC073A1"]
["Accessoires standard","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Alimentation électrique","Nom","","","","","V1"]
["","Phase","","","","","1~"]
["","Fréquence","","","Hz","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240"]