{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-S / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30S2V1B / RXTM30A2V1B","FTXTM40S2V1B / RXTM40A2V1B"]
["Puissance frigorifique","Min.","","kW","1.2","1.2"]
["","Nom.","","kW","3","4"]
["","Max.","","kW","4.6","5.2"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","0.8","0.9"]
["","Nom.","","kW","3.2","4"]
["","Max.","","kW","7.4","8.8"]
["Efficacité nominale","EER","","","5.13","4.71"]
["","COP","","","5.2","5.51"]
["","Consommation énergétique annuelle","","kWh","292","425"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","3","4"]
["","SEER","","","8.65","8.93"]
["","Consommation d’énergie annuelle","","kWh/a","121","157"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++","A+++"]
["","Puissance","Pdesign","kW","3","3.8"]
["","SCOP/A","","","5.2","5.5"]
["","Pdh Puissance calorifique à -10°","","kW","3","3.8"]
["","Consommation d’énergie annuelle","","kWh/a","807","967"]
["Remarques","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - See separate drawing for operation range","(2) - See separate drawing for operation range"]
["","","","","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]