{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Classe d'efficacité énergétique","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Puissance frigorifique","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Rafraîchissement de l'air ambiant","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","","","371","371","371","371"]
["","Puissance","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Classe d’efficacité énergétique","","","","","","","","","","","A++","A++","A++","A++"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Classe d’efficacité énergétique","","","","","","","","","","","A+","A+","A+","A+"]
["","Consommation d’énergie annuelle","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Efficacité nominale","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["Remarques","","","","","","","","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Voir le schéma séparé pour la plage de fonctionnement","(1) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","","","","","","","","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Pour les données électriques, se reporter au schéma séparé.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m.","(2) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","","","","","","","","","","835","835"]
["","COP","","","","","","","","","","","","","4.08","4.08"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","","","","","","","","","A","A"]
["","","Chauffage","","","","","","","","","","","","A","A"]
["Puissance calorifique","Nom.","","kW","","","","","","","","","","","7.50","7.50"]
["Remarques","","","","","","","","","","","","","","(3) - Voir le schéma séparé pour la plage de fonctionnement","(3) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","","","","","","","","","","(4) - Pour les données électriques, se reporter au schéma séparé.","(4) - Pour les données électriques, se reporter au schéma séparé."]