{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L9V1B","FVQ100CVEB / RZQG71L9V1B","FVQ100CVEB / RZQG100L9V1B","FVQ140CVEB / RZQG100L9V1B","FVQ125CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG140L9V1B"]
["Puissance frigorifique","Nom.","","kW","6.8","","9.5","","12.0","","13.4"]
["Rafraîchissement des locaux","SEER","","","6.23","6.31","5.61","5.61","5.61","5.61"]
["","Consommation d’énergie annuelle","","kWh/a","383","378","593","593","749","749"]
["","Puissance","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Classe d’efficacité énergétique","","","A++","A++","A+","A+","A+","A+"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","6.33","6.33","11.30","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.20","3.87","3.87"]
["","Classe d’efficacité énergétique","","","A+","A+","A+","A+","A","A"]
["","Consommation d’énergie annuelle","","kWh/a","2,189","2,189","3,767","3,767","4,088","4,088"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","1,010","","1,245","","1,870","","2,085"]
["","EER","","","3.37","","3.81","","3.21","","3.21"]
["","COP","","","3.64","","4.14","","3.70","","3.61"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","","A","","A"]
["","","Chauffage","","A","","A","","A"]
["Puissance calorifique","Nom.","","kW","7.5","","10.8","","13.5","","15.5"]
["Remarques","","","","(1) - La consommation énergétique annuelle est conforme à la directive 2002/31/CE sur l'étiquetage énergétique.","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Les valeurs SEER et SCOP sont conformes à la norme EN 14825.","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]