{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.02","0.02","0.03"]
["","Chauffage","","Nom.","kW","0.02","0.03","0.03"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","600","600","600"]
["","","","Largeur","mm","750","750","750"]
["","","","Profondeur","mm","238","238","238"]
["Poids","Unité","","","kg","17","17","17"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","8.7","9.2","11.6"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7","7","9"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","4.9","4.9","6.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1","4.1","5.4"]
["","","Chauffage","Haut","m³/min","9.2","9.8","12.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","7.2","7.2","10"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.6","5.6","8.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1","4.1","5.9"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","52","53","61"]
["","Chauffage","","","dBA","52","53","62"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","38","39","44"]
["","Refroidissement","","Moyen","dBA","32","32","38"]
["","","","Bas","dBA","25","25","31"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","20","27"]
["","Chauffage","","Haut","dBA","38","39","46"]
["","","","Moyen","dBA","32","32","40"]
["","","","Bas","dBA","25","25","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","29"]
["Réfrigérant","Réfrigérant-=-PRP","","","","675","675","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.4","6.4","6.4"]
["","Gaz","","DE","mm","9.5","9.5","12.7"]
["","Évacuation","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Télécommande câblée","","","","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240"]