{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":8,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM50B2V1B","FVXM35B2V1B (Archived)"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.02","0.03","0.02"]
["","Chauffage","","Nom.","kW","0.02","0.03","0.03"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","600","600","600"]
["","","","Largeur","mm","750","750","750"]
["","","","Profondeur","mm","238","238","238"]
["Poids","Unité","","","kg","17","17","17"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","8.7","11.6","9.2"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","7","9","7"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","4.9","6.6","4.9"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1","5.4","4.1"]
["","","Chauffage","Haut","m³/min","9.2","12.8","9.8"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","7.2","10","7.2"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","5.6","8.4","5.6"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.1","5.9","4.1"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","52","61","53"]
["","Chauffage","","","dBA","52","62","53"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","38","44","39"]
["","Refroidissement","","Moyen","dBA","32","38","32"]
["","","","Bas","dBA","25","31","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","20","27","20"]
["","Chauffage","","Haut","dBA","38","46","39"]
["","","","Moyen","dBA","32","40","32"]
["","","","Bas","dBA","25","35","25"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","29","19"]
["Réfrigérant","Réfrigérant-=-PRP","","","","675","675","675"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.4","6.4","6.4"]
["","Gaz","","DE","mm","9.5","12.7","9.5"]
["","Évacuation","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Télécommande câblée","","","","BRC073A1","BRC073A1","BRC073A1"]
["Accessoires standard","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Alimentation électrique","Nom","","","","V1","V1","V1"]
["","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240"]
["Remarques","","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS, 24 °CBH ; longueur équivalente de tuyauterie : 5m","(1) - Rafraîchissement: temp. intérieure 27°CBS, 19°CBH; temp. extérieure 35°CBS, 24°CBH; longueur équivalente de tuyauterie : 5m"]
["","","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m","(2) - Chauffage: temp. intérieure 20°CBS; temp. extérieure 7°CBS, 6°CBH ; tuyauterie équivalente de réfrigérant : 5m"]
["Accessoires standard","FVXM50B2V1B","","","","","1"]