{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F"]
[]
[]
[]
[]
["","","","","FVXS25FV1B (Archived)","FVXS35FV1B (Archived)","FVXS50FV1B (Archived)"]
["Niveau de pression sonore","Chauffage","Haut","dBA","38","39","45"]
["","","Faible niveau sonore de fonctionnement","dBA","23","24","32"]
["","","Bas","dBA","26","27","36"]
["","Rafraîchissement","Faible niveau sonore de fonctionnement","dBA","23","24","32"]
["","","Bas","dBA","26","27","36"]
["","","Haut","dBA","38","39","44"]
["","","Nom.","dBA","32","33","40"]
["","Rafraîchissement","Nom.","dBA","32","33","40"]
["Accessoires standard","Manuel d'installation","","","1","1","1"]
["","Manuel d’utilisation","","","1","1","1"]
["","Télécommande infrarouge","","","1","1","1"]
["","Piles","","","2","2","2"]
["","Support de télécommande","","","1","1","1"]
["","Flexible d'évacuation","","","1","1","1"]
["","Filtre purificateur d’air","","","","1","1"]
["","Bande d'isolation thermique","","","2","2","2"]
["Systèmes de contrôle","Infrared remote control","","","ARC452A1","ARC452A1","ARC452A1"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.52","12.7"]
["","Évacuation","","","20","20","20"]
["Sound power level","Rafraîchissement","","dBA","52","52","60"]
["","Chauffage","","dBA","52","52","60"]
["Dimensions","Unité","Largeur","mm","700","700","700"]
["","","Profondeur","mm","210","210","210"]
["","","Hauteur","mm","600","600","600"]
["Caisson","Couleur","","","Blanc","Blanc","Blanc"]
["Poids","Unité","","kg","14","14","14"]
["Power supply","Phase","","","1~","1~","1~"]
["","Fréquence","","Hz","50","50","50"]
["","Nom","","","V1","V1","V1"]
["","Tension","","V","220-240","220-240","220-240"]
["Remarques","","","","(1) - 220V","(1) - 220V"]
["","","","","(2) - 230 V","(2) - 230 V"]
["","","","","(3) - 240V","(3) - 240V"]
["Accessoires standard","Filtre purificateur d'air","","","2"]
["Remarques","","","","(4) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder."]