{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":77,"n_cols":11,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXT-ATV3CL"]
[]
[]
[]
[]
["","","","","","FWXT10ABTV3CL","FWXT15ABTV3CL","FWXT20ABTV3CL","FWXT10AATV3CL (Archived)","FWXT15AATV3CL (Archived)","FWXT20AATV3CL (Archived)"]
["Dimensions","Unité","","Largeur","mm","","","","902","1,100","1,300"]
["","","","Profondeur","mm","","","","128","128","128"]
["","","","Hauteur","mm","","","","335","335","335"]
["Casing","Colour","","","","","","","RAL 9003","RAL 9003","RAL 9003"]
["Poids","Unité","","","kg","","","","14.0","16.0","19.0"]
["Power supply","Phase","","","","","","","1~","1~","1~"]
["","Fréquence","","","Hz","","","","50","50","50"]
["","Tension","","","V","","","","230","230","230"]
["Puissance frigorifique","7/12°C","","Min.","kW","0.49","0.62","0.70"]
["","","","Moy.","kW","0.88","1.08","1.21"]
["","","","Max.","kW","1.24","1.61","1.94"]
["Puissance frigorifique sensible","7/12°C","","Min.","kW","0.37","0.52","0.57"]
["","","","Moy.","kW","0.70","0.86","1.02"]
["","","","Max.","kW","0.98","1.27","1.52"]
["Puissance calorifique","45/40°C","","Min.","kW","0.55","0.79","0.74"]
["","","","Moy.","kW","1.00","1.36","1.55"]
["","","","Max.","kW","1.50","2.01","2.13"]
["Puissance absorbée","Min.","","","kW","0.01","0.01","0.01"]
["","Moy.","","","kW","0.01","0.01","0.01"]
["","Max.","","","kW","0.02","0.02","0.03"]
["Vitesse de ventilation","Min.","","","tr/min","680.00","680.00","680.00"]
["","Moy.","","","tr/min","1100.00","1100.00","1100.00"]
["","Max.","","","tr/min","1500.00","1500.00","1500.00"]
["Caisson","Couleur","","","","RAL 9003","RAL 9003","RAL 9003"]
["","Matériau","","","","Tôle","Tôle","Tôle"]
["Dimensions","Unité","","Hauteur","mm","335","335","335"]
["","","","Largeur","mm","902","1102","1302"]
["","","","Profondeur","mm","128","128","128"]
["","Unité emballée","","Hauteur","mm","490","490","490"]
["","","","Largeur","mm","1030","1230","1430"]
["","","","Profondeur","mm","210","210","210"]
["Poids","Unité","","","kg","14","16","19"]
["","Unité emballée","","","kg","15","17","20"]
["Emballage","Matériau","","","","Carton","Carton","Carton"]
["","Poids","","","kg","1","1","1"]
["Échangeur de chaleur","Quantité","","","","1","1","1"]
["","Volume interne de serpentin","","","l","0.5","0.61","0.77"]
["","Charge","","Pression de service","bar","10","10","10"]
["Circuit d'eau","Diamètre des raccords de tuyauterie","","","in","3/4","3/4","3/4"]
["","Matériau de tuyauterie","","","","CUIVRE","CUIVRE","CUIVRE"]
["","Pression","Chauffage","Max.","bar","10","10","10"]
["Circuit d’eau - chute de pression d’eau","Chauffage","45/40°C","Min.","kPa","5.10","4.81","6.00"]
["","","","Moy.","kPa","12.00","6.30","6.40"]
["","","","Max.","kPa","16.30","7.20","8.10"]
["","Rafraîchissement","7/12°C","Min.","kPa","4.80","4.70","5.50"]
["","","","Moy.","kPa","10.50","5.60","5.40"]
["","","","Max.","kPa","11.70","5.10","5.30"]
["Circuit d’eau - débit d’eau","Chauffage","45/40°C","Min.","kg/h","100.00","140","150.00"]
["","","","Moy.","kg/h","170.00","240","300.00"]
["","","","Max.","kg/h","260.00","350","420.00"]
["","Rafraîchissement","7/12°C","Circuit d’eau - débit d’eau-=-Rafraîchissement-=-7/12°C-=-Min.-=-kg/h","kg/h","80.00","110","120.00"]
["","","","Moy.","kg/h","150.00","190","210.00"]
["","","","Max.","kg/h","210.00","280","330.00"]
["Niveau de puissance sonore","Min.","","","dBA","35","36","37"]
["","Moy.","","","dBA","46","47","48"]
["Niveau de puiss. sonore","Max.","","","dBA","53.0","54.0","55.0"]
["Plage de fonctionnement","Chauffage","Côté eau","Min.","°C","30","30","30"]
["","","","Max.","°C","85","85","85"]
["","Rafraîchissement","Côté eau","Min.","°C","5","5","5"]
["","","","Max.","°C","18","18","18"]
["","Installation des unités intérieures","Temp. ext.","Min.","°CBS","0","0","0"]
["","","","Max.","°CBS","45","45","45"]
["Systèmes de commande","Télécommande infrarouge","","","","Pour FWXT-ATV3(C)(CL)","Pour FWXT-ATV3(C)(CL)","Pour FWXT-ATV3(C)(CL)"]
["","Intégré sur l'unité intérieure","","","","Oui","Oui","Oui"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230","230","230"]
["Consommation électrique","Max.","","","W","19","20","29"]
["","Veille","","","W","3","4","5"]
["Courant","Courant de fonctionnement maximum","","Chauffage","A","0.16","0.18","0.24"]
["","Courant de service max.","","Rafraîch.","A","0.16","0.18","0.24"]