{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":5,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-P7H"]
[]
[]
[]
[]
["","","","","FXMQ50P7VEH"]
["Réfrigérant","Type","","","R-410A"]
["Puissance frigorifique","Nom.","","kW","5.6 (1)"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35"]
["","","Type","","Raccord à dudgeon"]
["","Gaz","DE","mm","12.7"]
["","","Type","","Raccord à dudgeon"]
["","Évacuation","","","VP25 (I.D. 25/O.D. 32)"]
["Vide de faux-plafond requis >","mm","","","350"]
["Dimensions","Unité","Largeur","mm","1,000"]
["","","Profondeur","mm","700"]
["","","Hauteur","mm","300"]
["Caisson","Matériau","","","Tôle en acier galvanisé"]
["","Couleur","","","Non peint"]
["Poids","Unité","","kg","35"]
["Ventilateur","Pression statique extérieure - 60 Hz","Haut","Pa","200"]
["Hauteur manométrique","mm","","","625"]
["Panneau décoratif","Poids","","kg","4.5"]
["","Modèle","","","BYBS71DJW1"]
["","Dimensions","Hauteur","mm","55"]
["","","Profondeur","mm","500"]
["","","Largeur","mm","1,100"]
["","Couleur","","","Blanc (10Y9/0,5)"]
["Puissance calorifique","Nom.","","kW","6.3 (2)"]
["Power supply","Phase","","","1~"]
["","Fréquence","","Hz","50/60"]
["","Nom","","","VE"]
["","Tension","","V","220-240/220 +/-10%"]
["Remarques","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","(2) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]