{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":11,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GM R290"]
[]
[]
[]
[]
["","","","","","BGM0870Y1ACA","MGM1280Y1ACA","MGM2210Y1ACA","MGM2210Y1WAA","BGM0870Y1WAA","MGM1280Y1WAA"]
["Puissance frigorifique","Basse température","R-290","Nom","kW","0.871","","","","0.871"]
["","Moyennes températures","R-290","Nom","kW","","1.281","2.206","2.206","","1.281"]
["Caisson","Couleur","","Unité de condensation","","Gris","Gris","Gris","Gris","Gris","Gris"]
["Dimensions","Unité","","Hauteur","mm","735","735","830","830","735","735"]
["","","","Largeur","mm","400","400","620","620","400","400"]
["","","","Profondeur","mm","790","790","790","790","790","790"]
["Poids","Unité","","","kg","64","56","80","80","64","56"]
["Compresseur","Quantité","","","","1","1","1","1","1","1"]
["","Type","","","","Par compression de vapeur","Par compression de vapeur","Par compression de vapeur","Par compression de vapeur","Par compression de vapeur","Par compression de vapeur"]
["","Modèle","","","","NT2180UV","NEU6217U","NTX6225UV","NT6230U/CSR","NT2210U/CSR","NT6220U/CSR"]
["","Méthode de démarrage","","","","Directe","Directe","Directe","Directe","Directe","Directe"]
["Condenseur","Débit d'air","","","m³/h","600","600","1,200","1,200","600","600"]
["Defrost (dégivrage)","","","","","Gaz chauds","Gaz chauds","Gaz chauds","Gaz chauds","Gaz chauds","Gaz chauds"]
["Évaporateur","Pulsion d'air","","","m","4","4","4","4","4","4"]
["Plage de fonctionnement","Température de chambre froide","","Min.","°C","-25","-5","-5","-5","-25","-5"]
["","","","Max.","°C","-15","10","10","10","-15","10"]
["","Température extérieure","","Min.","°C","20","20","20","20","20","20"]
["","","","Max.","°C","45","45","45","45","45","45"]
["Réfrigérant","","","","","R-290","R-290","R-290","R-290","R-290","R-290"]
["","Réfrigérant-=-PRP","","","","3","3","3","3","3","3"]
["Alimentation électrique","Alimentation électrique-=-Tension-=-V","","","V","220-230","220-230","220-230","220-230","220-230","220-230"]
["","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","60","60","60","50","50","50"]