{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":7,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","HCU-PXB1"]
[]
[]
[]
[]
["","","","","","HCU2040PXB1","HCU4070PXB1"]
["Puissance frigorifique","Basses températures","","kW","kW","3.03","6.56"]
["Compresseur","Nombre de tours","","","tr/min","4,800","3,600"]
["Poids","Unité","","","kg","161","300"]
["Moteur de ventil.","Puissance","","","W","115","230"]
["","Entraînement","","","","EC","EC"]
["Échangeur de chaleur","Type","","","","Cu-Al standard.","Cu-Al standard."]
["Puissance absorbée","Basses températures","","Nom.","kW","3.79","7.05"]
["COP","Low temperature","","Nom.","","0.80","0.93"]
["Dimensions","Unité","","Largeur","mm","574","773"]
["","","","Profondeur","mm","1,452","1,684"]
["","","","Hauteur","mm","799","1,438"]
["Moteur de ventilateur 2","Sortie","","","W","115","230"]
["Caisson","Couleur","","","","Gris clair RAL 7035","Gris clair RAL 7035"]
["Ventilateur","Type","","","","Axial","Axial"]
["","Débit d'air","Rafraîchissement","Nom.","m³/min","63","126"]
["","Quantité","","","","1","2"]