{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":66,"n_cols":8,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHSCU-CM1"]
[]
[]
[]
[]
["","","","","","JEHSCU0200CM1","JEHSCU0250CM1","JEHSCU0300CM1"]
["Capacité de réfrig.","Temp. moyenne","R-407F","Nom.","kW","3.33","3.82","4.63"]
["Puissance frigorifique","Moyennes températures","R-449A","Nom","kW","3.33","3.82","4.73"]
["Capacité de réfrig.","Temp. moyenne","R-407A","Nom.","kW","3.48","4.09"]
["Puissance frigorifique","Moyennes températures","R-448A","Nom","kW","3.33","3.82","4.73"]
["Capacité de réfrig.","Temp. moyenne","R-134a","Nom.","kW","2.13"]
["Puiss. absorbée","Temp. moyenne","R-407F","Nom.","kW","1.74","2.09","2.65"]
["","","R-407A","Nom.","kW","1.59","1.99"]
["Puissance absorbée","Moyennes températures","R-448A","Nom","kW","1.65","1.98","2.56"]
["Puiss. absorbée","Temp. moyenne","R-134a","Nom.","kW","1.11"]
["Puissance absorbée","Moyennes températures","R-449A","Nom","kW","1.65","1.98","2.56"]
["COP","Moyennes températures","","R-448A","","2.02","1.93","1.85"]
["","","","R-449A","","2.02","1.93","1.85"]
["","Température moy.","","R-407F","","1.92","1.83","1.74"]
["","","","R-134a","","1.92"]
["","","","R-407A","","2.18","2.06"]
["Paramètres à pleine charge et à temp. ext. 32 °C (Point A)","Paramètres à pleine charge et à temp. ext. 32 °C (Point A)-=-R-134a","Paramètres à pleine charge et à temp. ext. 32 °C (Point A)-=-R-134a-=-Te -10 °C","Paramètres à pleine charge et à temp. ext. 32 °C (Point A)-=-R-134a-=-Te -10 °C-=-Puiss. frigorifique nominale (PA)-=-kW","kW","2.13"]
["Paramètres à pleine charge à temp. ext. 32 °C (Point A)","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-134a","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-134a-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-134a-=-Te -10 °C-=-Puissance absorbée nominale (DA)-=-kW","kW","1.11"]
["","","","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-134a-=-Te -10 °C-=-COP nominal (COPA)","","1.92"]
["","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407A","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407A-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407A-=-Te -10 °C-=-Puiss. frigorifique nominale (PA)-=-kW","kW","3.48","4.09"]
["","","","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407A-=-Te -10 °C-=-Puissance absorbée nominale (DA)-=-kW","kW","1.59","1.99"]
["","","","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407A-=-Te -10 °C-=-COP nominal (COPA)","","2.18","2.06"]
["","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407F","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407F-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407F-=-Te -10 °C-=-Puiss. frigorifique nominale (PA)-=-kW","kW","3.33","3.82","4.63"]
["","","","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407F-=-Te -10 °C-=-Puissance absorbée nominale (DA)-=-kW","kW","1.74","2.09","2.65"]
["","","","Paramètres à pleine charge à temp. ext. 32 °C (Point A)-=-R-407F-=-Te -10 °C-=-COP nominal (COPA)","","1.92","1.83","1.74"]
["Paramètres à pleine charge et temp. ext. 32 °C (Point A)","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-448A","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-448A-=-Te -10°C","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-448A-=-Te -10°C-=-Puissance frigorifique nominale (PA)-=-kW","kW","3.33","3.82","4.73"]
["","","","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-448A-=-Te -10°C-=-Puissance absorbée nominale (DA)-=-kW","kW","1.65","1.98","2.56"]
["","","","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-448A-=-Te -10°C-=-COP nominal (COPA)","","2.02","1.93","1.85"]
["","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-449A","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-449A-=-Te -10°C","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-449A-=-Te -10°C-=-Puissance frigorifique nominale (PA)-=-kW","kW","3.33","3.82","4.73"]
["","","","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-449A-=-Te -10°C-=-Puissance absorbée nominale (DA)-=-kW","kW","1.65","1.98","2.56"]
["","","","Paramètres à pleine charge et temp. ext. 32 °C (Point A)-=-R-449A-=-Te -10°C-=-COP nominal (COPA)","","2.02","1.93","1.85"]
["Paramètres à pleine charge à temp. ext. 25 °C","Paramètres à pleine charge à temp. ext. 25 °C-=-R-134a","Paramètres à pleine charge à temp. ext. 25 °C-=-R-134a-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 25 °C-=-R-134a-=-Te -10 °C-=-COP déclaré (COP2)","","2.21"]
["","Paramètres à pleine charge à temp. ext. 25 °C-=-R-407A","Paramètres à pleine charge à temp. ext. 25 °C-=-R-407A-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 25 °C-=-R-407A-=-Te -10 °C-=-COP déclaré (COP2)","","2.61","2.44"]
["","Paramètres à pleine charge à temp. ext. 25 °C-=-R-407F","Paramètres à pleine charge à temp. ext. 25 °C-=-R-407F-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 25 °C-=-R-407F-=-Te -10 °C-=-COP déclaré (COP2)","","2.46","2.33","2.21"]
["Paramètres à pleine charge et temp. ext. 25 °C","Paramètres à pleine charge et temp. ext. 25 °C-=-R-448A","Paramètres à pleine charge et temp. ext. 25 °C-=-R-448A-=-Te -10°C","Paramètres à pleine charge et temp. ext. 25 °C-=-R-448A-=-Te -10°C-=-Puissance absorbée (D2)-=-kW","kW","1.43","1.76","2.27"]
["","","","Paramètres à pleine charge et temp. ext. 25 °C-=-R-448A-=-Te -10°C-=-COP déclaré (COP2)","","2.53","2.32","2.23"]
["","Paramètres à pleine charge et temp. ext. 25 °C-=-R-449A","Paramètres à pleine charge et temp. ext. 25 °C-=-R-449A-=-Te -10°C","Paramètres à pleine charge et temp. ext. 25 °C-=-R-449A-=-Te -10°C-=-Puissance absorbée (D2)-=-kW","kW","1.43","1.76","2.27"]
["","","","Paramètres à pleine charge et temp. ext. 25 °C-=-R-449A-=-Te -10°C-=-COP déclaré (COP2)","","2.53","2.32","2.23"]
["Paramètres à pleine charge à temp. ext. 43°C","R-134a","Paramètres à pleine charge à temp. ext. 43°C-=-R-134a-=-Te -10 °C","Paramètres à pleine charge à temp. ext. 43°C-=-R-134a-=-Te -10 °C-=-COP déclaré (COP3)","","1.42"]
["Paramètres à pleine charge et temp. ext. 43°C","R-448A","Te -10°C","COP déclaré (COP3)","","1.31","1.36","1.31"]
["","R-449A","Te -10°C","COP déclaré (COP3)","","1.31","1.36","1.31"]
["Ventilateur","Type","","","","Axial","Axial","Axial"]
["Dimensions","Unité","","Hauteur","mm","662","662","662"]
["","","","Largeur","mm","1101","1101","1101"]
["","","","Profondeur","mm","444","444","444"]
["Poids","Unité","","","kg","69.7","71.7","73.7"]
["Réfrigérant","","","","","R-134a"]
["Caisson","Couleur","","","","Gris clair","Gris clair","Gris clair"]
["Réfrigérant","Réfrigérant-=-PRP","","","","1430"]
["","Type 2","","","","R-407A","R-407A"]
["","Type 3","","","","R-407F","R-407F","R-407F"]
["","Type 5","","","","R-448A","R-448A","R-448A"]
["","PRP type 5","","","","1387","1387","1387"]
["","PRP type 2","","","","2107","2107"]
["","PRP type 3","","","","1825","1825","1825"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","230","230","230"]
["Remarques","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque","(2) - Niv. de press. son. mesurée à 10m en chambre anéchoïque"]
["","","","","","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés.","(3) - Son fonctionnement repose sur des gaz à effet de serre fluorés."]