{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Accessoires standard","Manuel d'installation","","","","1"]
["","Manuel d’utilisation","","","","1"]
["","Tuyaux de raccordement","","","","1"]
["","Étiquette de réfrigérant pour réglementation F-gas","","","","1"]
["","Étiquette de charge de réfrigérant","","","","1"]
["","Étiquettes multilingues de gaz à effet de serre fluorés","","","","1"]
["Poids","Unité","","","kg","370"]
["Réfrigérant","Charge","","","TCO2Eq","24.0"]
["","PRP","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Type","","","","R-410A"]
["Moteur de ventilateur","Sortie","","","W","750"]
["","Entraînement","","","","Entraînement direct"]
["Échangeur de chaleur","Type","","","","Serpentin à ailettes transversales"]
["Dimensions","Unité","","Largeur","mm","1,240"]
["","","","Profondeur","mm","765"]
["","","","Hauteur","mm","1,680"]
["Caisson","Colour","","","","Blanc ivoire"]
["Ventilateur","Type","","","","Ventilateur à hélice"]
["","Débit d'air","Rafraîchissement","Nom.","m³/min","230"]
["","Quantité","","","","2"]
["Power supply","Phase","","","","3~"]
["","Fréquence","","","Hz","50"]
["","Tension","","","V","380-415"]
["Remarques","","","","","(1) - Mode priorité de rafraîchissement : temp. intérieure  27 °CBS,19 °CBH ; temp. extérieure 32 °CBS ; longueur de tuyauterie : 7,5 m ; dénivelé : 0 m"]
["","","","","","(2) - Mode priorité de rafraîchissement : temp. d'évaporation -10 °C ; temp. extérieure 32 °CBS ; Surchauffe d'aspiration : 10 °C"]
["","","","","","(3) - Mode récupération d'énergie à 100 % : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; charge de réfrigération 18 kW ; longueur de tuyauterie : 7,5 m ; dénivelé : 0 m"]
["","","","","","(4) - Température saturée de pression d'aspiration équivalente (côté réfrigération) : -10 °C (sous condition réfrigérée) ; puissance de raccordement pour unité de climatisation intérieure : 10 CV, avec une récupération d'énergie de 100 %"]
["","","","","","(5) - Compresseur 1"]
["","","","","","(6) - Compresseur 2"]
["","","","","","(7) - Compresseur 3"]
["","","","","","(8) - Charge usine de l'unité"]
["","","","","","(9) - Installer le siphon d'huile à 5 m de l'unité extérieure"]
["","","","","","(10) - Pour en savoir plus, se reporter au schéma de plage de fonctionnement."]
["","","","","","(11) - Pour en savoir plus sur les accessoires standard, se reporter au manuel d'installation/d'utilisation."]
["","","","","","(12) - Contient des gaz à effet de serre fluorés."]