{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-F"]
[]
[]
[]
[]
["","","","","","RXF50F5V1B","RXF20F5V1B","RXF25F5V1B","RXF35F5V1B","RXF42F5V1B"]
["Dimensions","Unité","","Hauteur","mm","610","556","556","556","556"]
["","","","Largeur","mm","923","740","740","740","740"]
["","","","Profondeur","mm","367","343","343","343","343"]
["Poids","Unité","","","kg","40","24","24","24","28"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10","-10","-10","-10"]
["","","","Max.","°CBS","48","48","48","48","48"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15","-15","-15","-15"]
["","","","Max.","°CBH","18","18","18","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","48","46","46","48","48"]
["","Chauffage","","Haut","dBA","49","47","47","48","48"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.8","0.42","0.42","0.55","0.75"]
["","Charge","","","tCO2Eq","0.54","0.28","0.28","0.37","0.51"]
["","Réfrigérant-=-PRP","","","","675","675","675","675","675"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","30","20","20","20","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","20","12","12","12","12"]
["Accessoires standard","Installation manual","","","","","1","1","1","1"]
["","Refrigerant charge label","","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","1","1","1"]
["","General safety precautions","","","","","1","1","1","1"]
["","Drain plug","","","","","1","1","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240","220-240"]
["Remarques","","","","","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés.","(1) - Contient des gaz à effet de serre fluorés."]
["","","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]