{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M"]
[]
[]
[]
[]
["","","","","","RXM20M2V1B","RXM25M2V1B","RXM35M2V1B","RXM42M2V1B","RXM50M2V1B","RXM50MV1B","RXM60M2V1B","RXM71M2V1B"]
["Dimensions","Unité","","Hauteur","mm","550","550","550","735","735","735","735","734"]
["","","","Largeur","mm","765","765","765","825","825","825","825","870"]
["","","","Profondeur","mm","285","285","285","300","300","300","300","320"]
["Poids","Unité","","","kg","32","32","32","47","47","44","44","56"]
["Compresseur","Type","","","","","Compresseur swing hermétique","","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10","-10","-10 (1)","-10 (1)","-10","-10","-10"]
["","","","Max.","°CBS","46","46","46","46 (1)","46 (1)","46","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CBH","18","18","18","18","18","18","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46","46","49","","","48","48"]
["","","","Nom.","dBA","","","","48","48","","","47"]
["","","","Bas","dBA","","","","","","44","44"]
["","Chauffage","","Haut","dBA","47","47","49","","","49","49"]
["","","","Nom.","dBA","","","","48","49","","","48"]
["","","","Bas","dBA","","","","","","45","45"]
["Réfrigérant","","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Charge","","","kg","0.76","0.76","0.76","1.30","1.40","1.4","1.45","1.15"]
["","Charge","","","tCO2Eq","0.5","0.5","0.5","0.88","0.95","0.9","1.0","0.78"]
["","Réfrigérant-=-PRP","","","","675","675","675","675","675","675","675","675.0"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","30","30","30","30","30","30","30","30.0"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","20","20","20","20","20","20","20","20.0"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","","","1","1"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Compresseur","Type","","","","Compresseur swing hermétique","","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique","Compresseur swing hermétique"]
["Accessoires standard","Drain plug","","","","","","","1","1","","","1"]
["Remarques","","","","","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","","","(1) - See separate drawing for operation range"]
["Accessoires standard","Drain cap","","","","","","","","","","","3"]