{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensions","Unité","","Hauteur","mm","870","870"]
["","","","Largeur","mm","1,100","1,100"]
["","","","Profondeur","mm","460","460"]
["Poids","Unité","","","kg","117","117"]
["Compresseur","Type","","","","Compresseur scroll hermétique","Compresseur scroll hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-20","-20"]
["","","","Max.","°CBS","46","46"]
["","Chauffage","Extérieure","Min.","°CBH","-20","-20"]
["","","","Max.","°CBH","15","15"]
["Sound power level","Rafraîchissement","","","dBA","73","76"]
["","Chauffage","","","dBA","76 (1)","79 (1)"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","53","57"]
["","Chauffage","","Nom.","dBA","60","63"]
["Réfrigérant","Type","","","","R-32","R-32"]
["","Charge","","","kg","5","5"]
["","PRP","","","","675","675"]
["Raccordements de tuyauterie","Liquide","","DE","mm","9.52","9.52"]
["","Gaz","","DE","mm","22.2","22.2"]
["","Longueur de tuyauterie","Max.","UE - UI","m","100","100"]
["","","Système","Préchargé d'usine jusqu'à","m","30","30"]
["","Charge de réfrigérant supplémentaire","","","kg/m","Voir le manuel d'installation","Voir le manuel d'installation"]
["Accessoires standard","Manuel d'installation","","","","1","1"]
["","Précautions générales de sécurité","","","","1","1"]
["","Attaches","","","","2","2"]
["","Étiquette F-Gas détachable","","","","1","1"]
["","Tuyaux de raccordement","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Fréquence","","","Hz","50","50"]
["","Tension","","","V","380-415","380-415"]
["Courant - 50 Hz","Intensité maximale de fusible (MFA)","","","A","20","20"]
["Remarques","","","","","(1) - Conforme à la norme ENER Lot 21","(1) - Conforme à la norme ENER Lot 21"]