{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H519W7"]
[]
[]
[]
[]
["","","","","BRC1H519W7."]
["Emballage","Matériau","","","Carton"]
["","Poids","","kg","0.0850"]
["Température extérieure","Humidité relative <","","%","95"]
["Dimensions","Unité emballée","Largeur","mm","217"]
["","","Hauteur","mm","50"]
["","","Profondeur","mm","161"]
["","Unité","Largeur","mm","85"]
["","","Profondeur","mm","25"]
["","","Hauteur","mm","85"]
["Caisson","Couvercle de boutons","","","non"]
["","Couleur","","","Blanc"]
["","DEL de fonctionnement","Couleur","","Blue status indicator"]
["Écran LCD","Type","","","100 x 150 dots"]
["","Rétroéclairage","Couleur","","Blanc"]
["","Dimensions","Largeur","mm","28.0"]
["","","Hauteur","mm","40.7"]
["Poids","Unité emballée","","kg","0.317"]
["","Unité","","kg","0.110"]
["Raccords de câblage","Longueur de câble","Max.","m","500"]