{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHBRD-ADY17 / ERRQ-AY1"]
[]
[]
[]
[]
["","","","","","EKHBRD011ADY17 / ERRQ011AAY1","EKHBRD014ADY17 / ERRQ014AAY1","EKHBRD016ADY17 / ERRQ016AAY1"]
["Puissance calorifique","Nom.","","","kW","11.3, 11.0, 11.2","14.5, 14.0, 14.4","16.0, 16.0, 16.0"]
["Puissance absorbée","Chauffage","","Nom.","kW","3.80, 4.40, 2.67","5.02, 5.65, 3.87","5.86, 6.65, 4.31"]
["COP","","","","","2.97, 2.50, 4.20","2.89, 2.48, 3.72","2.73, 2.41, 3.72"]
["Chauffage des locaux","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-SCOP","","2.96","2.98","3.01"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 55 °C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","A+","A+","A+"]
["","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-SCOP","","2.70","2.81","2.88"]
["","","","Chauffage des locaux-=-Sortie d'eau sous climat tempéré&nbsp;: 35&nbsp;°C-=-Général-=-Classe d'effic. saisonnière du chauffage d'ambiance","","C","B","B"]
["Remarques","","","","","(1) - EW 55°C; LW 65°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(1) - EW 55°C; LW 65°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(1) - EW 55°C; LW 65°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB"]
["","","","","","(2) - EW 70°C; LW 80°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(2) - EW 70°C; LW 80°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB","(2) - EW 70°C; LW 80°C; Dt 10°C; ambient conditions: 7°CDB/6°CWB"]
["","","","","","(3) - EW 30°C; LW 35°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB","(3) - EW 30°C; LW 35°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB","(3) - EW 30°C; LW 35°C; Dt 5°C; ambient conditions: 7°CDB/6°CWB"]