{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHTS-AC"]
[]
[]
[]
[]
["","","","","","EKHTS200AC","EKHTS260AC"]
["Dimensions","Unité","","Largeur","mm","600","600"]
["","","Hauteur","Ballon","mm","1,335","1,610"]
["","","","Intégré sur l'unité intérieure","mm","2,010","2,285"]
["","","","Profondeur","mm","695","695"]
["Caisson","Matériau","","","","tôle d'acier galvanisée (pré-découpée)","tôle d'acier galvanisée (pré-découpée)"]
["","Couleur","","","","Gris métallique","Gris métallique"]
["Réservoir","Étiquette énergie","","","","B","B"]
["","Matériau","","","","Acier inoxydable (EN 1.4521)","Acier inoxydable (EN 1.4521)"]
["","Perte de chaleur constante","","","W","50","63"]
["","Volume d'eau","","","L","200","260"]
["Poids","Unité","","Vide","kg","70","78"]